[image: ]INVITATION TO TENDER
Norwegian Refugee Council (NRC) invites bids from competent Construction Companies/Contractors in Iraq for the following works: "Constructions/Upgrading of Shelters inhabited by Syrian Refugees in Domiz Camp 1D” in Dohuk Governorate, Iraq, Kurdistan”- the work is to be undertaken on 93 shelter units; specifications and technical details are as follows:
	
	Location: Dohuk/Domiz Camp 1D
	
	

	
	BoQ for One House (WITH BASE)
	
	

	
	Description
	Unit
	Qty

	No
	Concrete Works
	
	

	CW-1
	Providing materials & equipment’s needed for concrete (1:2:4) to cast Housing Unit for living rooms with dimension (3.07*3.7) m and (3.08*3.7), with minimum thickness of 10cm (Cement should be Turkish made), and leveling the site till reach to zero with filling work and put plastic sheet before concrete works, and the concrete surface should be smoothed with needed equipment’s with taking in consideration the slope for water path, According to Technical Engineer recommendations.
	m3
	2.3

	Doors & Windows Works

	DW-1
	Provide & install reinforced Plastic Doors PVC (frame=6cm, panel=18cm, z=10cm), with dimension (1*2) m, the plastic materials should be Turkish made & not refurbished, with all the accessories needed (door lock, etc.). According to Technical Engineer Recommendations.
	Piece
	2

	DW-2
	Provide & install reinforced Plastic Windows PVC (Frame=6cm, Glass=4mm) with dimensions (1.0*1.0) m, the material should be Turkish made and not refurbished, with all the accessories needed, according to Technical Engineer Recommendations.
	Piece
	2

	
	Plastering Works

	PW-1
	Provide the materials and necessary tools of mortar for plastering walls inside the living rooms, with plastering frames of the doors and windows, mortar proportion should be 1:3 (Cement: Sand) and should be by 3 layers, the work is including of filling all the gapes from outside walls with all the accessories needed according to technical engineer recommendations.
	m2
	83

	
	Building work

	BW-1
	Provide the materials and necessary tools for leveling land with fill to build, by solid block (40*20*15) cm, with cement mortar 1:3, the first row of block should be put on 40cm face to level the (badillo) and the other rows on 15cm face and the opening of doors and windows is not exist in price, should be put iron lintels over doors and windows according to annex drawings and Technical Engineer recommendations.
	m2
	68

	
	Roofing Works

	RW-1
	provide the materials and necessary tools for installation of sandwich panels for the roof with dimension (4.4*7) m and (5) cm thickness fixing it on the walls by using possible screw and steel frame by cross section (4*8) cm and 2mm thickness with adding two steel same cross section at the middle of the roof, with all the accessories needed according to sketches and technical engineer recommendations.
	m2
	      31 

	
	Electricity Works

	EW-1
	Preparing, Installing, Connecting & Testing Light point, with (2x2.5 mm) electricity wire Turkish made and socket (40 A), & fixing the cable with walls by cable clips and should be Siemens type , with all the accessories needed, according to Plans & Technical Engineer recommendations.(Light=1 P)(2 m.l cable=1 P )(1 switch plug=1 P)(1 switch = 1 P)(1 Socket =2 P)
	Point
	20







	
	Location: Dohuk/Domiz Camp 1D
	
	

	
	BoQ for One House (WITHOUT BASE)
	
	

	No
	Description
	Unit
	Qty

	
	Doors & Windows Works

	DW-1
	Provide & install reinforced Plastic Doors PVC (frame=6cm, panel=18cm, z=10cm), with dimension (1*2) m, the plastic materials should be Turkish made & not refurbished, with all the accessories needed (door lock, etc.), according to Technical Engineer Recommendations.
	Piece
	2

	DW-2
	Provide & install reinforced Plastic Windows PVC (Frame=6cm, Glass=4mm) with dimensions (1.0*1.0) m, the material should be Turkish made & not refurbished, with all the accessories needed, according to Technical Engineer Recommendations.
	Piece
	2

	
	Plastering Works

	PW-1

	Provide the materials and necessary tools of morter for plastering walls inside the living rooms, with plastering frames of the doors and windows, the morter proportion should be 1:3 (Cement: Sand) and should be by 3 layers, the work is including of filling all the gapes from outside walls with all the accessories needed according to technical engineer recommendations.
	m2
	83

	
	Building work

	BW-1
	Provide the materials and necessary tools for leveling land with fill to build, by solid block (40*20*15) cm, with cement mortar 1:3, the first row of block should be put on 40cm face to level the (badillo) and the other rows on 15cm face and the opening of doors and windows is not exist in price, should be put iron lintels over doors and windows according to annex drawings and Technical Engineer recommendations.
	m2
	58

	
	Roofing Works

	RW-1
	Provide the materials and necessary tools for installation of sandwich panels for the roof with dimension (4.4*7) m and (5) cm thickness fixing it on the walls by using possible screw and steel frame by cross section (4*8) cm and 2mm thickness with adding two steel same cross section at the middle of the roof, with all the accessories needed according to sketches and technical engineer recommendations.
	m2
	   31 

	
	Electricity Works

	EW-1
	Preparing, Installing, Connecting & Testing Light point, with (2x2.5 mm) electricity wire Turkish made and socket (40 A), & fixing the cable with walls by cable clips and should be Siemens type , with all the accessories needed, according to Plans and Technical Engineer recommendations.(Light=1 P)(2 m.l cable=1 P )(1 switch plug=1 P)(1 switch = 1 P)(1 Socket =2 P)
	Point
	20


Essential Criteria for the Bidders
· Company profile indicating key personnel and their contact details.
· Evidence (certificates) of completing past construction projects.
· Volume of business done in last 3 years with evidence to confirm that.  
· Valid current license from KRI.
· Regulation on Registration, classification and grading of Contractors in Kurdistan
· Copy of bank statement of last 6 months.
Remark: The bids that do not meet the essential criteria will not be considered for evaluation.   
The bidders can receive the bidding documents only during office hours from 09:00 am to 15:00 pm - Sunday to Thursday; from the NRC office in Dohuk as per the address below: 
	Logistics Department 
Norwegian Refugee Council-Support Office 
ZRKA 99451, Bangawan Street 52st, Dohuk
Email Address: procurement.dohuk@nrc.no
Contact No: +964 (0)772 447 8742


[bookmark: _GoBack]The bids should be submitted within 10 days of this advertisement, before the office closing hours (16.30 pm) and the envelopes should be clearly marked – “"Constructions/Upgrading of Shelters inhabited by Syrian Refugees in Domiz Camp 1D” in Dohuk Governorate, Iraq, Kurdistan”- 93 shelter units
Late bids shall be rejected and no liability will be accepted for loss, late delivery or non-delivery, whatsoever. Bids shall be opened after 3 days of the last day of closing the bids at NRC Office in Dohuk 
NRC reserves the right to select/reject any bids, in part or full, as it may deem necessary. No liability or claim in that respect would be admissible or entertained whatsoever.  
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