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Section II: Schedule of Requirements
eSourcing reference: ITB/2016/180

A. Summary of Requirements 
[bookmark: _GoBack]UNOPS requirements are comprised of the following lots:
· Lot 1: Night Vision Binocular
· Lot 2: NVG Helmet Mount Kit

B. Technical specifications for Goods and Comparative Data Table

Lot No 1: Night Vision Binocular

	Item No
	UNOPS minimum technical requirements
	Quantity
	Is bid compliant? Bidder to complete
	Details of goods offered. Bidder to complete

	1
	Gen3 Auto gated configuration
	500
	☐ Yes   ☐ No
	Insert details of goods offered, including specifications and brand/model offered if applicable

	2
	Standard L-3 EOS Gen3 CS001 tubes or L-3 EOS Gen3 Filmless tube
	
	
	

	3
	Dimensions not more than : 4.5″(L) x 5″(W) x 3.5″(H)
	
	
	

	4
	Weight: not more than 23 oz.
	
	
	

	5
	Battery Type / life: One (1) Standard AA Battery / Approx. 10 Hours or Two (2) Standard AA Battery / Approx. 20 hours at Room Temp.
	
	
	

	6
	Waterproof: not less than 66′
	
	
	

	7
	Warranty: 1 Year Warranty
	
	
	

	8
	Resolution: not less than 64 lp/mm 
	
	
	

	9
	Sensitivity:1800uA/lm @2,856K Photocathode
	
	
	

	10
	Magnificaiton:1X
	
	
	

	11
	Field of View (FOV):40º
	
	
	

	12
	Objective: F/1.2
	
	
	

	13
	Diopter: +2 to -6
	
	
	

	14
	Focus Range: 9.8″ to Infinity
	
	
	

	15
	Adjustment: 52-80mm Interpupillary
	
	
	

	16
	Temp: -3 oC to 49 oC (Operating), -15.5 oC to 71 oC (Storage)
	
	
	

	17
	Gen3 Autogated configuration
	
	
	

	18
	Two (2) Standard AA Batteries
	
	
	

	19
	Two (2) Eye Cup Assemblies
	
	
	

	20
	Soft Carry Case
	
	
	

	21
	Lens Tissue
	
	
	

	22
	Two (2) Sacrificial Windows
	
	
	

	23
	Two (2) Demist shields
	
	
	

	24
	Operator’s Manual
	
	
	



Lot No 2: NVG Helmet Mount Kit

	Item No
	UNOPS minimum technical requirements
	Quantity
	Is bid compliant? Bidder to complete
	Details of goods offered. Bidder to complete

	1


	Lock Release Lever allows NVG height to be easily adjusted up or down, then secured.
	500
	☐ Yes   ☐ No
	Insert details of goods offered, including specifications and brand/model offered if applicable

	2
	A Breakaway Release Lever allows the operator to easily set the desirable mode (breakaway or locked), depending upon operational needs.
	
	
	

	3
	An ergonomically placed Flip Release Button allows the Mount to “flip up” to a stowed position when the goggle is attached.
	
	
	

	4
	A Tilt Adjustment Knob allows the operator to fine adjust the tilt angle of the NVG.
	
	
	

	5
	A Mount Release Lever allows attachment and removal of the mount.
	
	
	

	6
	A Fore/Aft Release Lever allows for fore/aft travel of the goggle. Releasing the lever allows the operator to set the fore/aft position of the goggle.
	
	
	

	7
	An ergonomically placed NVG Release Button allows for one handed release of the NVG.
	
	
	

	8
	A Three Hole Shroud with Lanyard fits MICH/ACH and Crye Airframe style helmets
	
	
	

	9
	Material Construction Light Weight, Aerospace Grade Metal
	
	
	

	10
	Accommodates NVG AN/PVS-7B and 14 (Both Require Optional Hardware), 7A, 7C, 15, and 18
	
	
	



C. Delivery requirements and Comparative Data Table

	UNOPS Requirements
	Is bid compliant? Bidder to complete
	Details 
Bidder to complete

	Delivery time
	Bidder shall deliver the goods   2 Weeks after Contract signature.
	☐ Yes   ☐ No
	Insert details 

	Delivery place and Incoterms rules
	Erbil Airport - Iraq
	☐ Yes   ☐ No
	Insert details 

	Consignee details
	TBC
	☐ Yes   ☐ No
	Insert details 

	UNOPS Right to vary requirements
	At the time the Contract is awarded, UNOPS reserves the right to vary the quantity of the goods and associated services specified above, provided this does not exceed +/- [20%] , without any change in the unit prices or other terms and conditions of the ITB.
	☐ Yes   ☐ No
	Insert details 





D.  Inspections and tests 
The following inspections and tests shall be performed: 

The vendor must have the goods inspected in the manufacturer’s works by a competent authority and submit a test certificate and also a guarantee/warranty certificate that the goods conform to written specifications.
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