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REQUEST FOR QUOTATION

From: NRC, Hamam Al Alil Office, near MSF old hospital Hamam Al Alil 	
Date: 15th Nov 2017 		
No. of pages including this page: RFQ 6 Pages.

Subject: 	Construction Work for Market in Hamam Al Alil IDPs Camps 2.
PR Reference number: 554/11/HAA

Manner of Submission: 
Please submit your quotation in accordance with the requirements to NRC sub-offices located in Mosul, Hamam Al-Alil, Erbil and Baghdad. The office addresses are as below. 

In sealed envelope in the RFQ box with clearly mark the RFQ 554/11/HAA to 

· NRC, Hamam Al Alil Office near old MSF hospital Hamam Al Alil. 
· NRC Erbil office, Ekhlas Empire Building,3rd Floor, Korani Ainkawa Area, 100 Meter Street.
· NRC Mosul office, Al-Majmua Takafiya Area, East Mosul.  

[bookmark: _GoBack]Deadline for submission of quotations is <01:00PM Iraqi Time on Monday 20th Nov 2017> promptly. Companies who do not submit their quotation by this deadline will not be considered. 

Requirements:
The office of the Norwegian Refugee Council invites your company to make a firm offer for the following items
Goods: Services 
Specifications: As per below table 
Quantity: As per below table 











	#
	Item
	Unit
	Quantity Required
	Price Per Unit (USD)
	Total Price per Facility (USD)
	Facilities Required
	Total Price for All Facilities (USD)
	Notes

	1
	Supply of materials & installation of shed of 3 m height, 10 m length,5m width.
To include installation (welding) of outer frame of steel poles 3"*1.5" each 1m, into two directions.  Inner frame is of 1.5"*1.5" steel poles.
All fixed to a steel pole column of  2"*2" each 3m, 40 cm fixed to the ground by concrete base.a Steel pole to be fixed on the side walls with a height of 0.75m and 1.5m from the top.
outer frame only covered with kerby sheet, type 07 (thickness 3mm or higher).  Colour to be chosen by supervisor engineer.  Inclusive of all required fittings.
	m^2
	50
	 
	 
	3
	 
	5*20

	2
	Supply of materials & installation of shed of 3 m height, 15 m length, 5m width.
To include installation (welding) of outer frame consisting steel poles 3"*1.5" each 1m, into two directions.  Inner frame is of 1.5"*1.5" steel poles.
All fixed to a steel pole column of  2"*2" each 3m, 40 cm dug into the ground by concrete base.  Steel pole to be fixed on the side walls with a height of 0.75m and 1.5m from the top.
outer frame only covered with plastic kerby sheet, type 07 (thickness 3mm or higher).  Colour to be chosen by supervisor engineer.  Inclusive of all required fittings.
	m^2
	75
	 
	 
	3
	 
	6*50

	3
	Supply of materials & install partitions of plywood (12mm) of 2 m width and 3 m in hight , one sided and 5cmx5 cm thickness 2mm hollow galvanized steel frame, including fixing single parts and fixing at ground and the steel frame.a dood from the same materials of 2*1 to be installed and a window of 1.2*1 and ventilation opening of 50*50 cm . 
For Material&Items, acceptable country of origin: Galvanized Sheet:Ukranian, Plywood: Malaysian
	m^2
	150
	 
	 
	3
	 
	2





Please Note: All required material must be as per standard of below Bill of Material. If any defects or substandard material supplied that will be rejected by NRC site engineer. 

	Item
	Specification

	sand 
	The sand used shall be free of cohesive blocks and harmful foreign substances such as salts and organic matter  . It must be approved by the Supervisor Engineer, and the water must be used in all types of concrete . Clean construction of dirt as well as dirt, salts and organic matter and according to general technical conditions and instructions And the actual water content of concrete cement shall not exceed 60%, samples should be taken and should be subjected to the specified test .  its specifications is according to the Iraqi standards and (125 C - ASTM) . place of origin : Iraq / Karbala , Kalak

	cement
	The cement used shall be of a new type of Portland approved by the Supervisor Engineer and filled in . For the foundations and parts buried below the earth level. samples should be taken and should be subjected to the specified test , its specifications.is according to the Iraqi standards and (125 C - ASTM) . place of origin : Iraq / Sulimania

	gravel
	The gravel used for mix concrete must be clean of impurities, dust and mud as it should be Contains the appropriate gradient and be of the type that gives concrete with resistance and durability acceptable.samples should be taken and should be subjected to the specified test , its specifications.is according to the Iraqi standards and (125 C - ASTM) . place of origin : Iraq 

	mixed concrete
	Provide the required concrete from the factories approved for pre cast concrete by the Iraqi Standards and Metrology And with the consent of the supervisor and in the case of small quantities (less than 5 cubic meters) or if it is not possible ,  concrete ( or as required by the work stage) The concrete is mixed in situ and is the responsibility of the machine Mixing, labor, and mixing materials shall be provided by the Contractor, provided that the concrete shall be subject to inspection in all cases.  samples should be taken and should be subjected to the specified test according to the Iraqi specifications and American standards (109 C ASTM)

	Ply wood
	should be of new ,  clean and dry sheet of 12 mm in thickness , black in color . Place of origin is Malyssia . Sample should be submitted.

	steel tube
	should be of new , clean , painted with anti corrosion paint . Place of origin is Ukrain . Sample should be submitted . 

	Kerby sheet
	should be consist of 5 laeyrs : top coat , corrosion resistance primer , pre treatment layer , Zinc-Aluminium coating and high tensile strength steel . Of excepted source of origin






Delivery location: Hamam Al Alil IDPs Camp s 
( GPS Coordinates of Camp Location: Longitude: 43° 14' 16.898" E(43.238027)
Latitude: 36° 9' 14.871" N(36.154130)

Your quotation should clearly indicate the following;
· Currency of offer should be USD 
· Ex-works unit price:
· Transport cost up to delivery place: by air, sea, land (as applicable):
· Total price (INCOTERM Delivered Duty Unpaid (DDU) if the goods is delivered by an international supplier):
· Net price after deduction of discounts:
· Confirmed delivery schedule:
· Validity of the offer (Preferably 30 days)
· Defects liability and guarantee period: 1 month 
· Detailed specifications (if different from stipulated specifications):
· Place of manufacture and country of origin: As per attached Bill of Material.





Conditions of quotation:
Payment will be made within 30 days of receipt of goods, by bank transfer/cheque only. 

NRC is not subject to VAT; therefore all offers should be exclusive of VAT costs. 


All suppliers doing business with NRC should maintain high standards on ethical issues, respect and apply basic human and social rights, ensure non-exploitation of child labour, and give fair working conditions to their staff. NRC reserves the right to reject quotations provided by suppliers not meeting these standards. 
Vendors doing business with NRC will be screened on anti-corruption due diligence before NRC confirms an order or contract.

NRC aims to purchase products and services that the minimum environmental impact. Environmental considerations form part of the NRC selection criteria, and NRC reserves the right to reject quotations provided by suppliers not meeting these standards. 

Currencies of bid and payment
All prices shall be quoted by the Bidder in (USD) unless otherwise stated. Similarly, all payments will be made in <. USD.>). 

Inspection 
NRC is obliged to ensure that its procurement decisions are clearly justified and documented and keeping within the Donors mandatory principles. In that regard, full and on-the-spot access must be granted to representatives of NRC, the Donor or any organisation or person mandated by it, to premises belonging to NRC or its contractors. The right to access shall include all documents and information necessary to assess, or audit the implementation of the contract











Supplier Information

Company name………………………………………………Stamp…………………………...

Address…………………………………………………………………………………...............

Contact person……………………………………………………………………………………

Contact Telephone number……………………………………………………………………..

Email/Fax………………………………………………………………………………………….

NRC reserves the right to accept or reject the whole or part of your quotation based on the information provided. Incomplete quotations which do not comply with our conditions will not be considered. 

Shortlisted suppliers will be required to submit samples of each item. Please be sure to have all samples available at short notice, and wait for a response from NRC if you have been shortlisted.
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