[image: ]                              REQUEST FOR QUOTATION


RFQ Title: Shelter Kits
RFQ Submission Deadline: 15th November 2018, 16:00/Human Relief Foundation, Dream City Villa 29, Erbil, Iraq
RFQ Ref#: HRFRFQSHKT01080518

Summary:
Vendors are invited to submit a quotation for 32,250 shelter kits, to contain the following items:


	Item
	Minimum Specifications
	Unit
	Quantity

	Steel timber nails
	65 mm
Size: 8d
Small Galvanized Nail
100% HDG/ hot dip galvanized steel in accordance with ASTM-A153
Headed nail
Approximate quantity per kilo: 200 - 250
	kg
	1

	Clear plastic sheets
	190 GSM (gram per square meters)
Dimensions: 6*4m
	piece
	2

	Expanding spray foam
	Polyurethane Multipurpose Foam
Application temperature from  +4°C to +45°C
Expansion capacity 50% of original volume or higher
Closed cells, R-value 6 or higher.
Tack Free Time 5-15min at 21C
Curing Time 50-100 min
Cutting Time 50-100 min
Density 18-25 kg/m3
Fire Behaviour: Class B3
Joint sound insulation 58dB
Temperature Resistance From -40°C - +90°C
Shelf life of 15 months after delivery
In accordance with FEICA minimum standard
	tube
	4

	Nails with washer head
	2.70mm × 70mm
Nails with washer head / roofing nail
100% HDG/ hot dip galvanized steel in accordance with ASTM-A153
Washer in rubber with ardox body
10d / 18x30 (JPxLPP) / 2 ¾ x 10 (Inch x BWG)
Approximate quantity per kilo: 50
	kg
	1

	Binding wire
	Roll of binding wire, 1.8-2.5mm thickness; 30m long
	roll
	1

	Galvanized concrete nails
	4.00 mm x 80mm
Size: 12d 
High quality carbon steel, zinc plated
With smooth shank and round cap
	kg
	0.5

	Duct tape
	Polyethylene film over cloth scrim and rubber adhesive Length 54.8m – Width 48mm 
Adhesion to Steel: 62~72 oz./in. width (79 N/100 mm) 
Ref: D-3330
Tensile Strength: 19 ~32 lbs./in. width (560 N/100 mm)
Ref: D-3759
Elongation at Break: 15% ~ 24% Ref: D-3759
Thickness: 5.8~8.1 mils (0.147-0.21 mm) 
Ref: D-3652
Temperature Use Range: Up to 200°F (93°C)
	roll
	1



	Saw
	Carpenter all-purpose – standard coarse cut saw
2D/3D teeth type
Blade in forged steel, BD2/BS4659
Handle in hardwood
Blade material: spring steel 
Blade size: 20" (508mm)
Blade thickness: 1mm 20"""" Standard Coarse Cut Saw
Total length: 750mm
Teeth per Inch: 7~9 pt.
	piece
	1

	Utility knife
	Folding Retractable Utility Knife
Blade Length 100~150mm
Handle Length 150mm
Color: dark color
Number of blades: minimum 3
Handle in rubber covered metal or hard plastic
Style: Retractable
Weight: 0.15~0.25kg
	piece
	1

	Caulk gun
	10 oz metal ratcheting caulk gun
	piece
	1

	Silicone caulking tube
	100% clear, 10 oz tube
	tube
	2

	L-shaped galvanised steel angle
	42x42x40mm 
Thickness 2 mm
	piece
	4

	Flat L-corner 
	Galvanized Steel 
50mm x 50mm / 5cm x 10cm metal plates with screws
	piece
	4

	Metal handle for door
	Zinc or Aluminium, with screws (for wood) 10 to 15 cm length
	piece
	2

	Hinges with screws
	For door installation
	piece
	4

	Latch
	Galvanised steel: 6mm diam and 5-10 cm long
	piece
	2

	Open shackle padlock
	60mm, with keys
	piece
	2

	Exterior grade plywood
	Size: 12mm thick x 1.21m x 2.42m
OSB/3 – Load bearing board for humid conditions
Density (ρ): 450-500 (kg/m3)
Bending strength - major axis (EN 310) : 20N/mm3
Bending strength - minor axis (EN 310) : 10N/mm3
Modulus of elasticity in bending - major axis (EN 310) : 3500N/mm3
Modulus of elasticity in bending - minor axis (EN 310) : 1400N/mm3
Internal bond (EN 319) : 0.32N/mm3
Swelling in thickness in 24h (EN 317) : 15%
Dimensional change at 1% change in panel moisture content: 0.02 (Length %), 0.03 (Width %), 0.05 (Thickness %)
Approximate Moisture Content (20oC/85% humidity): 15%””
	piece
	4

	Torch
	3 LED Dynamo Wind Up Flashlight Hand Press Crank NR No Battery Torch Light Specifications: Color:Yellow/Red/Blue Material: Plastic Size:10×5×2.5cm
	piece
	1

	Screwdriver
	Drive type: crosshead/flathead- in-line with screws provided
Length: 150mm
Handle: plastic or wooden
	piece
	1

	Claw hammer
	Weight: min 750g
Handle: wooden
	piece
	1

	Square cut timber
	2cm x 6cm x 3m, rough cut, kiln dried lumber, 
	piece

	9

	Square cut timber 
	2.5 cm x 10cm x 300 cm, rough cut, kiln dried lumber, 
	piece

	4

	Bag
	CANVAS Tool bag, water resistance,  
	piece
	1



· HRF reserves the right to alter and amend the size and quantity of items listed above.
· HRF reserves the right to accept bids in part or in full.

Submission Requirements:
1. Detailed BoQ - stamped
2. Detailed pricing, and price breakdown - stamped
3. Printed BoQ and pricing - no handwriting
4. Completed itemised spreadsheet.
5. No correction pen on any document
6. Proposals in sealed envelopes
7. Place a CD containing soft copies of the documents in the envelope
8. Put the RFQ title, ref# and vendor name on the envelope and CD
9. Put the RFQ ref# and name on each page of your quotation 
10. No email submission
11. [bookmark: _gjdgxs]Quotation currency: United States Dollars.
12. If the submission deadline falls on a weekend or holiday, the next working day will be the new deadline
13. Interested vendors should submit all the required documents to HRF's Erbil Office. Address: Human Relief Foundation, Dream City Villa 29, Erbil, Iraq.

[bookmark: _30j0zll]Payment:
1. All HRF payments are made within 30 days of correct invoice submission
2. Correct invoices are submitted only after satisfactory completion of the work and GRN signing
3. Payment methods: bank transfer or cheque (bank transfer is preferred)
4. No cash payment under any circumstances
5. The vendor is responsible for any bank charges from their end
6. The vendor is responsible to provide a bank account that works with HRF’s bank in Iraq

Vendor Registration:
1. Unregistered vendors are required to complete their registration before the end of the submission deadline
2. Vendors that fail to register on time will not be considered in the opening session 
3. To complete vendor registration, please see the attached Vendor Registration form in this advertisement

Samples:
1. HRF may request samples of proposed items for testing, samples won’t be returned to the vendors unless stated otherwise by HRF in writing
2. Samples must be clearly marked to indicate the RFQ and vendor name
3. A list of samples and their serials, if available, to be submitted with the samples
4. All samples must be placed in appropriate boxes and delivered to HRF office as per instructions
5. Sample requests are made prior to award
6. If any lab test is required, the vendor will be liable for the test cost 






Other:
1. Bonds: not required at the RFQ stage
2. Site visits: not required 
3. Pre-proposal meeting: not available
4. Technical data: required where applicable
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