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[bookmark: _Hlk9251761]                       LOT 1 – Workshop Tools

	No.
	Item name
	Description
	Quantity
	Reference Picture

	1
	Workshop Tool Trolley                 عربة ادوات الورشة

	· Empty trolley dimensions Approx. (1000h x 1070w x 460d mm)
· Drawers: min. 10 drawers
· Material: Metal
· Rigid design with work top. 
· Side plates with holes to attach accessories. 
· Rubber corners for impact protection. 
· Heavy duty transport for comfortable steering content label on each drawer or similar product.
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	2
	Portable Engine Stands                               حامل المحرك

	· Approx. Dimensions: 90*40*17
· Material: Steel
· Movable engine stands with a net weight of 40-60 Kg 
· Capable of lifting 900-1100Kg smoothly and safely with gearbox 
· Universal Fit, 4-point Universal Mounting Brackets that Fits Most Engines
· Practicality, 360º Swiveling & Locking Wheels for Easy Maneuverability and Extra Stability
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	3
	Air Compressor                     ضاغط الهواء
	· Discharge / Operating Pressure: min. 10 bar
· Dimension Approx.: 1600*575*1090MM
· Horse Power: min 10hp
· Min. 350 lt. capacity
· Belt driven single stage twin cylinder compressor. The compressor has two quick – action couplings. One coupling for regulated pressure and one for full, unregulated tank pressure  
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	4
	Battery Charger Station
(Middle)                            "محطة شاحن البطارية
الوسطية"

	· Input Voltage 220V.                                 
· Instant electric current 1250A -1450 A Force start, slow and fast charge 12-24 v  
· Protection device for over loading and short circuit. Display for voltage and current. Unique automatic monitor for voltage and current.  Time regulation system with high accuracy. 
· Double - layer bridge communication. With fast charge & slow charge (12/24). (HUA) curve silicon steel chip 100% copper core transformer. 
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	5
	Brake Fluid Tester Pen                       قلم فحص سائل الفرامل

	· Auto Power off, 1 LR03 AAA Battery 
· Size: 15-19cm Length (Approx.)
· Material: Plastic
· Weight: Approx. 150-250g
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	6
	Parallel Vice Swivel Large           ملزمة رابطة ذات قطب متوازي كبير (منكنة)

	· Bench Vice. 
· All steel
Fixed / Swivel Base
Casted Iron
Painted Body approx. 6inch
· Jaw Opening: approx. 6 inch
Jaw Width: 6”.
· Approx. Dimensions: 40 x 23 x 20.6 cm
 
	12
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	7
	Air Impact Wrench                       مفتاح براغي انج

	· Screwdriver: approx.1 inch 
· Bolt Capacity: approx. 45mm
· Max. Torque min. 1800ft.lb (2,445Nm)
· Net Weight approx.: 10.61kg
· Length approx. :537mm
· Air cons approx.: 0.85m3 /min
· Air Inlet :1/2 inch
· Air Pressure approx. :90-115 Psi 
· Sound Pressure: max. 98dBA Vibration: max. 9.6m/S 2 
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	8
	Hand Pallet Jack Wide Forks جك يدوي نقال

	· Approx.2 Ton load capacity
· Wide forks standard with fork width of approx. 600- 685 mm and length of 100-1.22m
	24
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	9
	Manual Hydraulic Press منصة الضاغط الهيدروليكي  اليدوي

	· 10 ton Stand    
· Material: Iron
· Height approx.: 2-2.5m
· Width approx.: 1.2-1.6m
· Movable piston, 
· overload safety valve, double speed control unit, pressure gauge, 
· manual up/down control unit 10-20 ton 
	12
	[image: E:\Wurth Cataloge Tools\Catalog  Photo\Electro Hydrulic.JPG]

	10
	Pneumatic Axle Jack جاك هوائي محور العجلة

	· Two stage pneumatic jack with approx. 100-111mm height at 80ton +93mm at 50 ton and min height of 255mm 
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	11
	Axle Stand حامل محوري
	· Min. 20 Ton Heavy Duty jack stand with max height of 1.05M and minimum height of 675mm 
· Dimensions: 12 x 12 x 14.5 inches
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	[bookmark: _Hlk9159856]12
	Crawler Board                                  عربة او نقال زاحفة

	· Capacity approx.: 140 -200 Kg.
· Weight approx.: 7-11 Kg
· Color approx.: Orange or Red
· Dimension approx.: 40-42” L 15-17” W & 4”H
· Caster wheels: min. Six Rotating Caster wheels with 3-5” Inch
· Padded seat & Headers for ultimate comfortable 
· Practical gap for the tool’s storage Easy cleaning
	48
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	13
	Stand Drill                         دريل ثابت ملم
	· Drill stand cast iron base, Size approx.: ᴓ43mm,
· Volts approx. / hz 230 - 240 volt / 50 hz 1000W
· Hight approx.: 1800-2000mm
· Depth adjustment scale for drilling depth 150-200mm
· Three speeds with the safety switch off
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	14
	Grinder                                كوسرة مع حمالة واط
	· Approx. Volts / hz 230 - 240 volt / 50 hz  RPM 2000-2800 
· wattage 550W -1000W 
·  Bench top grinding machine complete with 200mm grinding
·  wheel grade 60 and grade 30
·  preferable with bench grinder stand 
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[bookmark: _Hlk9251738]                       LOT 2 – Safety Equipment’s

	No.
	Item name
	Description
	Quantity
	Reference Picture

	1
	First Aid Kits                           حقيبة اسعافات اولية

	First aid, middle size 
This kit contains:
Scissor 1 Pc
Dettol Liquid 1 Pc
Paracel 500 Tab 1 Pc
Nicip Tab 1 Pc
Cotton 15 gm 1 Pc
Micropore 1 Inch
Betadine Point 15g
Burnell Cream 10gm
Lop amide Tab 1 Pc
Soft swab 10 cmx 10 cm
Bandage (3m/10cm) 1 Pc, with all necessary medical needs.
	24
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	2
	Fuel fire extinguisher type                 مطفأة حريق امكافحة حرائق الوقود
	Are fires involving flammable liquids such as fuel, size 6-12 liter with expiry date more than 1 year. The origin must be similar to EU standards or other equivalent standards.
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	3
	Electrical fires extinguisher type                 مطفأة حريق امكافحة حرائق الكهرباء
	Are fires caused by electricity, size 6-12 liter with expiry date more than 1 year. The origin must be similar to EU standards or other equivalent standards.
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LOT 3  – Truck Tire Equipment’

	No.
	Item name
	Description
	Quantity
	Reference Picture

	1
	Truck Tire Changer                        مغير اطار الشاحنة
	Portable console, for wheel with a max Diameter of 1.5M wheel width up to 1M, 8.5 thickness rein forced plates on the lifting arm 130-150 bar, 
Rim diameter 14 inch to 26 inches. 

	12
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	2
	Truck Wheel Balance                        موازن عجلة الشاحنة           
	Tier lifter. Have 3 kinds of ALU mode and STA mode, two different function for cars and trucks 1.2M max width of 512mm
Power Supply: 220V
Wheel weight: 100-160kg
Imbalance Resolution: ±1g/±10g
Working ambient: 5°C-40°C
Noise: <70db.
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Remarks
1) [bookmark: _Hlk9324260]Bidder can apply for all LOTS or One LOT individually.
2) Minimum 1 years warranty period for all goods are required. Please specify.
3) All reference pictures are not an indication for any specific brand but only to understand the description.
4) [bookmark: _GoBack]All dimensions and physical characteristics are approximate not exact.
5) Supplier must submit Technical Data Sheet / catalogue or brochures of offered product (Please specify the exact model). 
6) DAP, Baghdad (Iraq).  
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