ANNEX E: LIST OF BRANDS AND ORIGINS 
Title of the Action: Restoration of Peace, Livelihoods and Economic Cycles in Anbar (RePLECA) – Rehabilitation of Al-Falaq school/ Anbar-Heet

	N
	ITEM
	DETAIL
	BRAND OFFERED

	Part1) Civil Works

	1.12
	Internal/external walls and fence Painting
	Supply materials, lobar force, and machinery to paint the external and internal walls of the building within three layers of painting each layer 0.4-2 mm Jotun or equivalent. The price includes repairing cracks using plastic/steel wire mesh on cracks area and ensuring of well levelling of the walls vertically and horizontally and corners as well with all requirements to accomplish the work as per the instructions of supervisor engineer.
	

	1.14
	1.2 m Ceramic Cladding
	Supply materials, labor force, and machinery to clad the classrooms walls with ceramic European quality or equivalent up to height of 1.2 m with cement mortar 1:3. The price includes filling joints with white cement. The samples brands and colors should be approved by supervisor engineer with all requirements to accomplish the work as per the instructions of supervisor engineer.
	

	1.15
	Acoustic Gypsum false ceiling (60*60 cm)

	
Supply materials, labor force, and machinery to install false ceiling acoustic (Saudi type) or equivalent for classrooms. The price includes fixing galvanized steel sections (H-sections-beams) every 60 cm, inverted T-section (Black Sika), screw and fisher, and with all requirements to accomplish the work as per the instructions of supervisor engineer.
	

	1.18
	Aluminium windows
	Supply materials and labor force to install aluminium windows (2*1.7 M) *12 and (1.2*1.7) *1 turkey made asistal or equivalent slide or fixing based on the instructions of supervisor engineer. The price includes installation of iron frame of channel 4 inches and 3 mm thickness during the masonry works then painted with two layers of anti-rust and proper final painting, glass 6 mm, rubber, handles, hinges, anti-flees for movable windows, and with all requirements to accomplish the work as per the instructions of supervisor engineer.
	

	Part2) Plumping Works

	2.6
	PVC Pipes
	Supply and install (6") dia PVC pipes Egyptian origin or equivalent to be connected between the toilets to the septic tanks. The price includes provision and installation of all required fittings with all requirements to accomplish the work as per the instructions of supervisor engineer.

	

	Part 3) Electrical Works

	3.0
	Copper wires
	The copper wires used in all electrical connections.
	

	3.1
	Sub-Distribution board 12 lines (Including all its details)
	Supply materials and labor force to install Sub-Distribution board 12 lines. The board should include circuit breakers and three phase changeover/conductors with capacity 200-amp Schneider or equivalent using cable 4*35 mm2 for connections between main board and Sub-Distribution boards, insulators, switches and etc., all items should be arranged properly, affords a high degree of safety operation, with all requirements to accomplish the work as per the instructions of supervisor engineer.
	

	3.2
	Main Switch Board (M.S.B.) (Including all its details)

	
Supply, install, and connect M.S.B Dimensions 120 cm x 80 cm x 40cm using rubber gaskets and equipped with the following items and Bus bars 600A 4No with earth bus bar, the price also includes the required relays, timer, and finder protection device or equivalent. and 1 Piece of Volt- and Amperemeter and 3 pcs. Signal lamps and 1 set Copper Bus-Bar 1000A with length 100 Cm, insulators, switches etc., all items should be arranged properly, affords a high degree of safety operation.
Note: Main Circuit breaker and Sub- Circuit breakers should be LEGRAND or Group Schneider or ABB original mark or equivalent.
	

	3.3
	4*35 mm2 cable connection
	Supply electrical cable size 4*35 mm2 reinforced Saudian origin or equivalent to be connected from the main electrical source to M.D.B, then to S.D.B. The price includes affixing properly either by hidden pipes through masonry works or through galvanized tray cable with all requirements to accomplish the work as per the instructions of supervisor engineer.
	

	3.4
	Switch Socket, 13 A, 230 V
	Supply, connect and operate electrical point with electrical Plug switch of 13 Amp capacity made in Europe or equivalent using single copper wires (3x2.5) mm2. The price includes establishments the electrical wires through 25 mm PVC pipes through slabs and walls during works and galvanized steel box with all requirements to accomplish the work as per the instructions of the supervising engineer.
	

	3.5
	Switch Socket, 32 A, 230 V
	Supply, connect and operate electrical point with electrical Plug switch of 13 Amp capacity made in Europe or equivalent using single copper wires (3x4) mm2. The price includes establishments the electrical wires through 25 mm PVC pipes through slabs and walls and galvanized steel box with all requirements to accomplish the work as per the instructions of the supervising engineer.
	

	3.6



	60*60 Drop Ceiling LED 96 Watts Light
	Supply, connect and operate 60*60 drop ceiling light 96 Watts Turkish brand Nextlite or equivalent using single copper Saudian (2*1.5) mm2. The price includes establishments of wires through masonry and concrete slab using 25 mm PVC pipes with using galvanized box in the wall and PVC junction inside concrete slab, in addition to using switches keys made in Europe or equivalent, with all requirements to accomplish the work as per the instructions of supervisor engineer.

	

	3.7
	Wall Mounted Waterproof LED Lights
	Supply, connect and operate circular waterproof LED lights 75 Watts Turkish brand Nextlite or equivalent using single copper Saudian (2*1.5) mm2. The price includes establishments of wires through masonry and concrete slab using 25 mm PVC pipes with using galvanized box in the wall and PVC junction inside concrete slab, in addition to using waterproof switches keys made in Europe or equivalent, with all requirements to accomplish the work as per the instructions of supervisor engineer.
	

	3.8
	Energy Save Light LED 75 Watts
	Supply, connect and operate   LED lights 75 Watts fluorescent Turkish brand Nextlite or equivalent using single copper Saudian (2*1.5) mm2. The price includes establishments of wires through masonry and concrete slab either by excavating and re-plastering or by using exterior 20 mm PVC pipes from S.D.B to the light points with using galvanized box in the wall and PVC junction inside concrete slab, in addition to using switches keys French origin Schneider or equivalent, with all requirements to accomplish the work as per the instructions of supervisor engineer.
	

	3.9
	Projector LED Flood Light
	Supply, connect, and operate wall lights 250-watt Turkish origin Nextlite or equivalent halogen lamp or LED using copper wires Saudian or equivalent (2*4) mm2. The price includes establishments of wires through masonry either by excavating walls and re-plastering or by using exterior galvanized tray cable from the S.D.B to the projector points, iron pipes to be installed on a higher level, in addition to using waterproof switches keys French origin Schneider or equivalent, with all requirements to accomplish the work as per the instructions of supervisor engineer.
	

	3.10
	60*60 Ceiling fan
	Supply, connect and operate drop ceiling fan Panasonic brand or equivalent using single copper Saudian (2*1.5) mm2. The price includes establishments of wires through masonry and concrete slab using 25 mm PVC pipes with using galvanized box in the wall and PVC junction inside concrete slab, in addition to using waterproof switches keys French origin Schneider or equivalent, with all requirements to accomplish the work as per the instructions of supervisor engineer.
	

	3.11
	Air cooler device 3 Ton Capacity
	Supply, connect, and operate air cooler ground-standing 3 tons capacity (3600 BTU) three phases of heating and cooling R410 economic and environmental (Tossot) or equivalent using (3*4) mm2. The price includes establishment of wires through walls and slabs during works using 25 mm PVC pipes, establishment of drainage system inside walls, installation of electrical device, Circuit 60-amp MCB three phase, key 45 Amp, with all requirements to accomplish the work as per the instructions of supervisor engineer.
	

	4.5
	Electric air ventilator
	Supply, connect, and operate air ventilator with size of 6 inches HES, Nexan, Prysmian or equivalent. The price includes using copper wires of (3*1.5) mm2 with electrical keys made in Europe or equivalent, with all requirements to accomplish the work as per the instructions of supervisor engineer.
	

	4.7
	Air cooler device 2 Ton Capacity
	Supply, connect, and operate air cooler with 2 tons capacity (24000 BTU) (TOSOT) or equivalent single phase of cooling and heating invertor R410 economic and environmental. The price includes using copper wires (3*4) mm2 to be stablished either by excavating and re-plastering or through exterior 20 mm PVC pipes from the S.D.B to the device, establishments of drainage system, circuit 45 Amp, key made in Europe or equivalent, with all requirements to accomplish the work as per the instructions of supervisor engineer.
	

	4.8
	Ceiling fan
	Supply materials and install ceiling fan "Panasonic" or equivalent, size 56 inch three blades, with safety hook, safety wire, safety screw, and safety fuse using copper wires (3*1.5) mm2 Saudian origin or equivalent. The price includes establishments of wires either by excavating through walls and slabs and re-plastering or by using exterior 20 mm PVC pipes from S.D.B to the points of fans, regulator using made in Europe or equivalent, with all requirements to accomplish the work as per the instructions of supervisor engineer.
	



NOTE: Some positions might include more than one items inside it such as boards and all the electrical positions which includes the item and its switches, please refer to the brands of all details.
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