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	Construction works
	Rehabilitation of Faluja Youth Forum

	Company name
	





	No.
	Material
	Item
	Description
	Acceptable range of quality
	Brand offered

	1
	Aluminum
	A - 2
	Supply materials and install new aluminum windows in different sizes and shapes (side opener casement and fixed panels) for the locations of above item (A- 1). Total profile depth should be not less than 4.5 cm, and the aluminum thickness not less than 1.8 mm. Samples and catalogues should be officially approved by the supervising engineer prior to implementation. Price includes installing double glass 6 mm each face with a void width of not less than 10 mm for the fixed panel, and not less than 16 mm for the side opener. Price also includes handles, hinges, anti-insect mesh, and all required accessories for the proper insulation of heat, damp, sound, and dust. All works should be done according to the drawings and the instructions of the supervising engineer.
	Alumex, Asistal, Amco, or equivalent
	

	
	
	A - 4
	Supply materials and install new aluminum doors (same sizes and locations as in the  above item) with aluminum thickness of 2mm. Samples and catalogues should be officially approved by the supervising engineer prior to implementation. Price includes knobs, lock hardware with keys, handles, hinges, and all accessories of the best quality. All works should be dome according to the specifications and instructions of the supervising engineer.
Note: in the doors which will be used as emergency exit, the interior handle should be a special emergency type (opens the door directly regardless of lock situation). Emergency doors are indicated in the drawings.
	Alumex, Asistal, Amco, or equivalent
	

	2
	Ceramic
	A - 19
	Supply materials and remove the damaged ceramic floors of the ground floor WCs with the mortar and dispose the rubble to the locations specified by the municipality. Then apply new ceramic tiles (30*30) cm, rough surface with all necessary works by a layer of sulphate resisting cement:sand mortar with mix ratio 1:3 according to instructions of site engineer. Price includes filling the joints with white cement and ensure curing for all the applied ceramics. Samples must be submitted by the construction company and approved by the supervising engineer prior to implementation.
	Itaca, Argenta, Luna tile, or equivalent
	

	
	
	A - 20
	Supply materials and Clad the walls with ceramic tiles (approved sample) using cement sand mortar with SBR with all necessary works according to instructions of site engineer. Price includes filling the joints with white Cement and ensure curing for all the applied Ceramics. Works of Ceramics should be leveled Horizontally and Vertically. All works should be dome according to the specifications and instructions of the supervising engineer.
	Itaca, Argenta, Luna tile, or equivalent
	

	3
	Wall paints
	A – 11
	Supply materials and paint the internal walls with three layers of paint. Type and color of paints should be officially approved by the supervisor engineer prior to implementation. Price includes treatment of walls' defects with paste according to specification and instructions of the site engineer.
	Jotun, Berger, Betek, or equivalent
	

	4
	Wooden doors
	A - 15
	Supply materials and remove the damaged doors' leaves (the frames to be kept), then install new interior wooden leaves, size (1.5*2.4)m. The door leaf should be made of 5mm thick wooden sheets, and the filling rectangular wood sections should be spaced at 5 cm intervals. Samples and catalogues should be officially approved by the supervising engineer prior to implementation. Price includes knobs, lock hardware with keys, handles, hinges, and all accessories of the best quality. All works should be done according to the specifications and instructions of the supervising engineer.
	Kian doors, Ikra doors, Zandoors, or equivalent
	

	5
	Handwash basin
	C - 7
	Supply materials and install handwash basin with stand, size 0.45 m x 0.45 m and sink height should be 0.8 m from the floor. The work includes high pressure connection steel hose, chromium plated stop valves, two angle valve, flex drain hose and all related accessories, and including connecting to the water and sanitary networks. With all needed works, Paper towel dispenser out of stainless steel. Samples must be submitted by the construction company and approved by the supervising engineer prior to implementation.
	Gerzo, Badella, Teko plus, or equivalent
	

	6
	Mixer tap
	C - 8
	Supply and install basin mixer tap with the following specifications:
- handle should be valve handle at a height of 0.90 m from the floor
- chrome color
- single hole installation
- not less than 35 mm ceramic cartridge
- not less than 120 mm between water outlet center and the mixer's body centerline
- Water Saving mousseur 5.7 l/min
- flexible connection hoses
- 55o lever rotation in each direction
All works should be done according to the instructions of the supervising engineer. Sample must be submitted by the construction company and approved by the supervising engineer prior to implementation.
	Grohe, Milano, Gerzo, or equivalent
	

	7
	Lights
	D - 1
	Supply materials and install LED panel light, 60*60 cm, for mounting in false ceiling, 60 W, AC 220-240 V, 50-60 Hz, white color, IP20. Price includes connection using single copper wires  (3x2.5) mm2, and pulling wires inside the PVC conduits and connecting it to the switches with all installation and connection accessories. All works should be done according to the drawings and the instructions of the supervising engineer. Samples must be submitted by the construction company and approved by the supervising engineer prior to implementation.
	Nextlite, BG, Raja, or equivalent
	

	
	
	D - 7
	Supply materials and install LED round downlight, for mounting in false ceiling, diameter not less than 210 mm, 18 W, AC 220-240 V, 50-60 Hz, 135 mA, white color, IP40, 25000 hours lifetime. Price includes connection using single copper wires  (3x2.5) mm2, and pulling wires inside the PVC conduits and connecting it to the switches with all installation and connection accessories. All works should be done according to the drawings and the instructions of the supervising engineer. Samples must be submitted by the construction company and approved by the supervising engineer prior to implementation.
	Nextlite, BG, Ozen, or equivalent
	

	8
	Exhaust fans
	D - 8
	Supply materials and install a 6-inch exhaust fan, round shape, auto shutter, 15 W, air discharge not less than 2.8 m3/min, 100% copper coil. Price includes connection using single copper wires  (3x2.5) mm2, and pulling wires inside the PVC conduits and connecting it to the switches with all installation and connection accessories. All works should be done according to the instructions of the supervising engineer. Samples and catalogues must be submitted by the construction company and approved by the supervising engineer prior to implementation.
	Nextlite, BG, Shami, or equivalent
	

	9
	Water heater
	D - 9
	Supply materials and install a wall mounted electrical vertical water heater, 45 L capacity, structure of 2 mm thick galvanized plate, double foam insulation, up to 8 bar pressure capacity. Price includes connecting to the switches using copper wires (3x4) mm2 according to the instructions of the supervising engineer, all necessary water pipes, safety valves, and shut valves for warm and cold water. the heater should be fixed according to the instruction and location selected by the supervising engineer. Samples must be submitted by the construction company and approved by the supervising engineer prior to implementation.
	Proline, Heatex, Thermex, or equivalent
	

	10
	AC
	D - 3
	supply, install, connect, and check split type air conditioner, wall mounted, cooling and heating, 12000 BTU cooling capacity, T3 class, single phase, invertor compressor, R410 Refrigerant, self cleaning function, turbo button, multi fan speeds, LED display, intelligent defrosting. Price includes fixing 1" diameter PVC or PPR pipes inside the walls for  AC condensate dewatering and connecting it to the nearest sewer by a gully trap, connecting the AC to the switches using single copper wires 3x4 mm2, and an electrical protection device. All works should be done according to the instructions of the supervising engineer. Sample must be submitted by the construction company and approved by the supervising engineer prior to implementation.
	GE, Gree, Tosot, or equivalent
	

	
	
	D - 4
	supply, install, connect, and check split type air conditioner, wall mounted, cooling and heating, 24000 BTU cooling capacity, T3 class, single phase, invertor compressor, R410 Refrigerant, self cleaning function, turbo button, multi fan speeds, LED display, intelligent defrosting. Price includes fixing 1" diameter PVC or PPR pipes inside the walls for  AC condensate dewatering and connecting it to the nearest sewer by a gully trap, connecting the AC to the switches using single copper wires 3x4 mm2, and an electrical protection device. All works should be done according to the instructions of the supervising engineer. Sample must be submitted by the construction company and approved by the supervising engineer prior to implementation.
	GE, Gree, Tosot, or equivalent
	

	
	
	D - 5
	supply, install, connect, and check split type air conditioner, floor stand, cooling and heating, 36000 BTU cooling capacity, T3 class, single phase, invertor compressor, R410 Refrigerant, self cleaning function, turbo button, multi fan speeds, LED display, intelligent defrosting. Price includes fixing 1" diameter PVC or PPR pipes inside the walls for  AC condensate dewatering and connecting it to the nearest sewer by a gully trap, connecting the AC to the switches using single copper wires 3x4 mm2, and an electrical protection device. All works should be done according to the instructions of the supervising engineer. Sample must be submitted by the construction company and approved by the supervising engineer prior to implementation.
	GE, Gree, Tosot, or equivalent
	

	
	
	D - 6
	supply, install, connect, and check split type air conditioner, cassette type, cooling and heating, 48000 BTU cooling capacity, T3 class, invertor compressor, R410 Refrigerant, self cleaning function, turbo button, multi fan speeds, LED display, intelligent defrosting. Price includes fixing 1" diameter PVC or PPR pipes for  AC condensate dewatering and connecting it to the nearest sewer by a gully trap, connecting the AC to the switches using single copper wires 3x4 mm2, and an electrical protection device. All works should be done according to the instructions of the supervising engineer. Sample must be submitted by the construction company and approved by the supervising engineer prior to implementation.
	GE, Gree, Tosot, or equivalent
	



Notes:
1- Bidders must submit origin of manufacture for all materials in the above list.
2- Bidders must submit brand with full product name and model number (ex: Schneider ComPact NSX100F)
3- Bidders must submit all catalogues (when applicable)
4- Samples should be provided by the bidders for physical checking (upon request of GIZ). In case of awarding, the samples will be kept in GIZ storage and released back to the company after completion of works.
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