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Compliance Statement of Specifications and Tender Terms

[bookmark: _Int_ukkwzp9N][bookmark: _Hlk116722545]It shall be the bidder’s responsibility to carefully examine the following sections and provide Items that are in compliance with the MAG (MINES ADVISORY GROUP) Minimum Requirements. 


	1. Technical minimum requirements of the Goods



 Diesel Fuel/ Minimum Standard Specification required
[image: ]

 Petrol Fuel/ Minimum Standard Specification required
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	# Lot
	Item(s) Description
	Specifications
	Average estimated monthly consumption in Litter
	Are you applying for this LOT? (YES/NO)

	1
	Diesel fuel to be delivered in Erbil 
	Flash point of 60°C and above for diesel fuel
	15000
	 

	
	Petrol fuel to be delivered in Erbil 
	Petrol should be unleaded with octane ratings of 93 and above
	5000
	 

	2
	Diesel fuel to be delivered in Chamchmal
	Flash point of 60°C and above for diesel fuel
	18000
	 

	
	Petrol fuel to be delivered in Chamchmal
	Petrol should be unleaded with octane ratings of 93 and above
	15000
	 

	3
	Diesel fuel to be delivered in Sulaymaniyah
	Flash point of 60°C and above for diesel fuel
	2000
	 

	
	Petrol fuel to be delivered in Sulaymaniyah
	Petrol should be unleaded with octane ratings of 93 and above
	2000
	 

	4
	Diesel fuel to be delivered in Chwarta
	Flash point of 60°C and above for diesel fuel
	2000
	 

	
	Petrol fuel to be delivered in Chwarta
	Petrol should be unleaded with octane ratings of 93 and above
	2000
	 

	5
	Diesel fuel to be delivered in Telkef
	Flash point of 60°C and above for diesel fuel
	15000
	 

	
	Petrol fuel to be delivered in in Telkef
	Petrol should be unleaded with octane ratings of 90 and above
	5000
	 

	6
	Diesel fuel to be delivered in Tel Afar
	Flash point of 60°C and above for diesel fuel
	10000
	 

	
	Petrol fuel to be delivered in in Tel Afar 
	Petrol should be unleaded with octane ratings of 90 and above
	10000
	 

	7
	Diesel fuel to be delivered in Sinjar 
	Flash point of 60°C and above for diesel fuel
	16000
	 

	
	Petrol fuel to be delivered in in Sinjar 
	Petrol should be unleaded with octane ratings of 90 and above
	6000
	 

	8
	Diesel fuel to be delivered in Duhok
	Flash point of 60°C and above for diesel fuel
	10000
	 

	
	Petrol fuel to be delivered in in Duhok
	Petrol should be unleaded with octane ratings of 93 and above
	6000
	 








Subcontractors and Third-Party Suppliers: Bidders must disclose any subcontractors or third-party suppliers involved in the process of fuel delivery to MAG Iraq. This includes any entities that will participate in or have a role in fulfilling the contract.
	Question
	Yes/No
	3rd Party details ( If Any)

	Do you have or willing to have any subcontractors or third-party suppliers that will be involved in the process of fuel delivery to MAG Iraq? If yes please provide details
	
	



	Supplier’s Premises Visit / Suppliers Meeting

	It is Required for this tender and will be scheduled by the Tender Committee - Yes



Shortlisted bidders which pass the technical evaluation stage will be visited for Due Diligence and capacity evaluation. During the visit the Committee will check the physical existence of the bidder and its office, Number of staffs, quality certification if any, evaluate the capacity to meet MAG’s delivery schedules. This includes assessing ability of the bidder to supply the required quantities to remote field bases efficiently.

	2. Purchase Terms



	TERMS
	COMPLIANCE
Yes/No

	
· Currency: The main currency of the Framework Agreement will be USD. Do you agree with USD being the currency of the agreement? 
	
Y/N?

	Delivery Terms: The supplier is fully responsible for delivering the goods in good quality to the MAG locations specified in the Tender Instructions File. This includes all aspects of the delivery process, such as loading, transportation, offloading, and a one-time Fuel Testing cost for each order.

If the delivery is handled by a third-party transport company, the supplier remains liable for the item until it is safely delivered to MAG’s premises and accepted by MAG. Detailed terms will be included in the framework agreement to clarify the point at which the supplier’s responsibility ends and MAG’s responsibility begins.
	Y/N?


	· [bookmark: _GoBack]Quotation Validity:  The cost quoted by the bidder shall be kept firm and unchanged for a minimum of 30 days. When the quotation’s issued date is not explicit, the deadline of the reception of the bids will be considered.
· In case the bidder does not agree with the above. How many days will the quotation be valid?

	Y/N?

Days: 


	· Payment Method: Bidder agrees to follow the MAG standard, 30 days after the reception of goods / services (Good Reception Note signature date) via bank cheque or bank transfer.
      If different payment method:
· Number of days after reception of the goods/services?

	Y/N?

Days:


	· Advance Payment. Bidder agrees with no advance payment as per MAG standards.

	Y/N?


	· The Bidder will not be permitted to take advantage of any errors or omissions in this Invitation to Tender or any Purchase Order or Contract thereafter. Should the Bidder discover any errors or omissions, the Bidder must notify MAG accordingly.

	Y/N?


	· Do you have a business registration with the Ministry of Trade in Federal Iraq?
	Y/N?

	· Do you have a business registration with the Ministry of Trade in Kurdistan Iraq Region (KRI)?
	Y/N?

	· Do you have a license of Oil services specialty from the Ministry of Natural Resources (Kurdistan Iraq Region)?
	Y/N?



Please note the MAG might shortlist/sign framework agreement with multiple suppliers/bidder and when required, the purchaser (MAG Iraq) shall ask for price quote on a monthly basis/need basis from the contracted suppliers, and issue the MAG purchase order to the best priced supplier. As the delivery of fuel will be required at multiple locations in Iraq (locations mentioned in the title of this tender) MAG Iraq will issue the purchase order/s to the most financially advantageous offer for that respective location. 

Bidder Comments, Detailed the Specific Terms in case they are different from MAG Terms
	








	3. Bidder Declaration




The Supplier’s representative accepts in full and without restriction the conditions governing this tender as the sole basis of this competition, whatever its own conditions of sale may be, which we hereby waive.
The Supplier’s representative has examined carefully, understood, and comply with all conditions, instructions, forms, provisions, and specifications contained in this tender dossier including the contract template with its annexes.
The Supplier’s representative is aware that failure to submit a tender containing all the information and documentation expressly required in the form requested and within the specified deadline, may lead to the rejection of the tender at MAG’s discretion.
The Bidder holds no reservation regarding the tender dossier; and are aware that any reservation may result in the rejection of the tender by MAG.

	Company name:  

Company’s Representative name:	 

Company’s Representative Job Title:	  

	  Representative’s signature 	 


  Company Stamp:
	

  City, date:	
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Test Discerption Unit Standard Specification

Specific Gravity @ 15°C (max) g/cem (0.850)

Flash Point (min) C 60

Total Sulfur Content (max) ppm 8000

Viscosity (cst) @40°C (max) st 5.6

Distilled @ 350 °C (min) %V 85

Appearance Clear & Bright

Water Content, Free %V NIy
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Test Discerption Unit Standard Specification
Specific Gravity @ 15.5C g/cem 0.710-0.775
Research Octane Number, RON Octane 93 Min for KRI

90 Min for FI
Motor Octane Number, MON Octane e
Total Sulfur Content Ppm wt 100 max
RVP(Range) Winter / Summer KPA 49-82 / 44-60
Benzene Vol% 1 max
Aromatics Vol% 35 max
Olefins. Vol% 18 max
Oxygen content Mass% 3.7 max
Initial Boiling Point, IBP (] Report
Final Boiling Point, FBP c 210 max

Appearance

Clear & Bright
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