 Subject:   Tender No.15 /T /TYN/2012  (imported) .
	 
 SupplyingPumps  Pscs(11)and Spare Parts   
 


The State Company for Tires Industries one of the companies of Ministry of Industry and Minerals announce making the tender No.15/ T /TYN/2012 for the new tire project  under classification ( A2,T5,D3,S1 ) within  the allocation of the investment plan 2012   so , the experienced & specialized  companies that have desire in participate to the tender have to visit the commercial department in the site of the company in     ( AL Najaf City – AL Haydariah ) or our office in Baghdad City at AL Saadon Street – AL Baraka Building in order to get the documents needed for participating in the tender against  un refundable sum ( 100000 ) one hundred  thousand Iraqi dinar .any offer which does not comply with the conditions will be neglected . note , the latest day to receive offers is 12A.M on  ( 20 /9 /2012 ) , offers should be presented to the secretary of the committee of opening offers against receipt supported the reception .offer should be attached with  ( 1% ) as bid bond from the offer amount  as a form of bank guarantee or as a approved cheque through a reliable Iraqi bank for Iraqi companies or as a bank guarantee from foreign bank accepted by and through  any reliable Iraqi bank  for non Iraqi companies otherwise the offer will be neglected , .The winner of the tender will endure the fees of publishing and advertising .for any information please visit our web site :
www.scti-iraq.com.
 Or the web site of the Ministry of Industry and Minerals :
  www.industry.gov.iq.   
	Item
	Tender No
	Closing date
	Description
	Quantity

	 1
	 15/T/TYN/2012 imported 
	 20/9 /2012
	Pumps pscs(11)andspare parts
	11 pumps  


      
Conditions of tenders and specifications
	Pump specification
	Pump type
	N

	NOTE
	QTY.
	sealing
	MOTOR
kw
	R.P.M
n-1
	T.water.
c
	H.
m
	Q.
M3/hr
	
	

	Cooling line for packing
Without motor
	2
	packing
	110
	2950
	180-200
	250
	105
	HPHW pump
	1

	Without motor
	1
	=
	250
	=
	25-27
	230
	200
	RO.Water pump
	2

	With motor
	1
	=
	18.5
	=
	75-90
	50
	90
	Boiler de aerator
vessel Pump
	3

	Compressor
Heat
Exchangers
With motor
	1
	=
	45
	=
	25-30
	60
	200
	Cooling Water
pump
	4

	With motor
	2
	=
	 
	=
	80-95
	140
	53
	condensate Pump
	5

	With motor
	1
	packing
	7.5
	2890
	10-70
	30.5
	9
	Seal water pump
	6

	With motor
	1
	=
	30
	1480
	25-30
	15
	500
	Intake water
pump
	7

	Without motor
	1
	=
	110
	1480
	25-30
	60
	450
	High lift water
pump
	8

	With motor
	1
	=
	30
	1480
	25-30
	50
	150
	Industrial waste
Water pump
 
	9


 

