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Section II: Schedule of Requirements
eSourcing reference: ITB-2016-181

A. Summary of Requirements

UNOPS requirements are comprised of the following lots:
· Lot 1: Handheld GPS
· Lot 2: Compasses

B. Technical specifications for Goods and Comparative Data Table

Lot No 1: Handheld GPS

	Item 
	UNOPS minimum technical requirements
	Quantity
	Is bid compliant? Bidder to complete
	Details of goods offered. Bidder to complete

	GPS Physical & Performance

	Unit dimensions, WxHxD: 
	Not more than 2.4" x 6.3" x 1.4" (6.1 x 16.0 x 3.6 cm) 
	80
	☐ Yes   ☐ No
	Insert details of goods offered, including specifications and brand/model offered if applicable

	Display size, WxH: 
	Not more than 1.6" x 2.2" (4.1 x 5.6 cm); 2.6" diag (6.6 cm) 
	
	
	

	Display resolution, WxH: 
	Not less than 160 x 240 pixels 
	
	
	

	Display type: 
	transflective, 65-K color TFT 
	
	
	

	Weight: 
	Not more than 9.2 oz (260.1 g) with batteries 
	
	
	

	Battery: 
	2 AA; NiMH or Lithium 
	
	
	

	Battery life: 
	16 hours 
	
	
	

	Waterproof: 
	IPX7 
	
	
	

	High-sensitivity receiver: 
	GPS & GLONASS
	
	
	

	Maps & Memory:

	Basemap & Ability to add maps
	
	
	

	4 GB Built-in memory
	
	
	

	Accepts microSD™  data cards 
	
	
	

	Waypoints/favorites/locations
	5000 
	
	
	

	Routes: 
	200 
	
	
	

	Track log: 
	10,000 points, 200 saved tracks 


	
	
	

	Features:

	Automatic routing (turn by turn routing on roads) with optional mapping for detailed roads
	
	

	Geocaching-friendly: paperless (250,000 preloaded, room for more)
	
	

	Custom maps compatible
	
	

	Photo navigation (navigate to geotagged photos)
	
	
	

	Hunt/fish calendar
	
	
	

	Sun and moon information
	
	
	

	Tide tables
	
	
	

	Area calculation
	
	
	

	Custom POIs (ability to add additional points of interest)
	
	
	

	online community where you analyze, categorize and share data
	
	
	



Lot No 2: Compasses

	Item No
	UNOPS minimum technical requirements
	Quantity
	Is bid compliant? Bidder to complete
	Details of goods offered. Bidder to complete

	1
	Direction Scale: Mils
	500
	☐ Yes   ☐ No
	Insert details of goods offered, including specifications and brand/model offered if applicable

	2
	Compass Accuracy: not less than 2 degrees
	
	
	

	3
	Compass Resolution: not less than 2 degrees
	
	
	

	4
	Balanced for northern and/or southern hemisphere
	
	
	

	5
	Clinometer
	
	
	

	6
	Large mirror 
	
	
	

	7
	Jewel bearing 
	
	
	

	8
	Adjustable declination correction scale 
	
	
	

	9
	Additional sighting hole for superior accuracy 
	
	
	

	10
	Baseplate with magnifying lens and anti-slip rubber pads
	
	
	

	11
	Detachable snap-lock in lanyard. Easy to detach for working with the map 
	
	
	

	12
	Wristlock in the lanyard
	
	
	

	13
	cm or inch scales
	
	
	

	14
	Measurements : not more than 65  x  101  x  18  mm 
	
	
	

	15
	Weight ; not more than 74 g
	
	
	

	16
	Bezel Material: Plastic
	
	
	

	17
	Metric scales cm, inch, 1:20 000 km Roamer, 1:25 000 km Roamer 
	
	
	

	18
	Balanced for northern hemisphere 
	
	
	

	19
	Declination correction adjustable
	
	
	



C. Delivery requirements and Comparative Data Table

	UNOPS Requirements
	Is bid compliant? Bidder to complete
	Details 
Bidder to complete

	Delivery time
	Bidder shall deliver the goods    2 Weeks after Contract signature.
	☐ Yes   ☐ No
	Insert details 

	Delivery place and Incoterms rules
	[bookmark: _GoBack]DAP: Erbil – Iraq- KRG Ministry of Peshmerga
	☐ Yes   ☐ No
	Insert details 

	Consignee details
	TBC
	☐ Yes   ☐ No
	Insert details 

	UNOPS Right to vary requirements
	At the time the Contract is awarded, UNOPS reserves the right to vary the quantity of the goods and associated services specified above, provided this does not exceed +/- 25%, without any change in the unit prices or other terms and conditions of the ITB.
	☐ Yes   ☐ No
	Insert details 





D.  Inspections and tests

The following inspections and tests shall be performed: 


The vendor must have the goods inspected in the manufacturer’s works by a competent authority and submit a test certificate and also a guarantee/warranty certificate that the goods conform to written specifications.

If the goods fail to meet the laid down specifications, the supplier shall take immediate steps to remedy the deficiency or replace the defective goods to the satisfaction of the purchaser.
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