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 PN 16.1850.3-001.00  

A. TECHNICAL SPECIFICATIONS OF Aluminum sulfate:
	
	Item Description
	Unit
	Quantity

	1.
	Aluminum sulfate, content of Aluminum Oxide (Al2O3) = 16.5-17 %
Appearance: Shall be clear to yellowish, dry, white solid and granulated form.

The aluminum sulfate shall be free of iron and shall not contain any impurities and additives.

The expire date shall not be less than 2 years from the date of producing.

Delivery: bags (30 kg up to 50 kg)

Terms and Conditions: presentation of original product certificate, provision of 1 kg sample before delivery, according to Iraq Technical Standard.

	Ton
	40




B. Remarks and Conditions 
	1
	Standard of products should be compliant with (Turkish, European or USA) standards or equivalent to international standards, all the product should be received and checked by related engineer for approval.

	2
	Unloading the bags of Aluminum Sulfate must be on wooden pallets, and covered by plastic sheets.

	3
	[bookmark: _GoBack]All items should be Delivered to directorate of water Duhok warehouse in Etit

	4
	Supplier must provide date of production after signing contract with origin company.

	5
	Product test must be succeeded in one of Kurdistan university lab'

	6
	Provide certificate of origin from production company.

	7
	Technical data sheet or specifications (catalogue) of the product should be attached to the offer documents

	8
	The delivery time must not exceed 10 days



1 | Page
image1.png
Deutsche Gesellschaft
fur Internationale
Zusammenarbeit (GIZ) GmbH




