ANNEX 1 - TECHNICAL SPECIFICATIONS
A. Technical Specifications

	Item No
	Product Name
	Product Specifications
	Quantity
	Unit
	Possible Producer, Equivalent brand and Reference Picture

	



1.
	Grass cutter machine vehicle
	Engine:  B & S Intek V-Twin cylinder 656cc European standards or Equivalent
Cutting Deck Size: Approx. 122cm/48in
Transmission: Hydrostatic
Blade Engagement Clutch: Electromagnetic
Discharge: Rear discharge with the option to mulch and
discharge (with optional accessories)
Cutting Positions: 7 positions, 30 – 90mm
Wheels: Approx. 15in x 18in
Grass box Capacity: 300 liters
Fuel Tank Volume: 7 liters
Net Weight: not less than 225 kg
	5
	pcs
	[image: Image result for SOLO t20-105.5]

	

2.
	Grass cutter machine manually
	TYPE: GEAR TYPE, European standards or Equivalent
Power: Approx. 6.25 HP                                    Engine: fuel, Briggs & Stratton 625 or equivalent                                                    Cutting width: Approx.  51cm                                                           workable surface: 2000 m2
	10
	pcs
	[image: Image result for SOLO 5235 sp-a]

	3.
	Manual plug & rotitler
	Engine:  fuel type, Briggs & Stratton 625 European standards or Equivalent.             
Displacement: Approx. 190 ccm 2.4 kW 2900 rpm, 
Waorking width = 50 cm                      
Tiller blades: 4 units Φ 30                                weight = Approx. 46 kg                                            (forward & Reverse) drive
	3
	pcs
	[image: Image result for alco mh 5001 r]

	4
	Hedge Trimmer
	Engine: fuel- 2 stroke, European standards or Equivalent                                  displacement: Approx. 23 cm3                                            power: Approx. 0.58kW/0.78 hp                               weight: Approx. 4.6 kg                                                           blade length: 60 cm                                                blade type: diamond cut
	9
	pcs
	[image: Image result for alko ht 700]

	5
	Chainsaw
	Engine: fuel, European standards or Equivalent                                                            displacement: Approx. 45.1 cm3                                                     power: Approx. 2.2kW/3.0 hp                                     power to weight ratio: Approx. 2.1kg/kW                           weight: Approx. 4.7 kg                                                 bar length: Approx. 38 cm
	3
	pcs
	[image: Image result for solo 646]




B. DELIVERY TIME AND DELIVERY LOCATION

-    The Delivery Location is GIZ's warehouse in Sulaymaniyah City.
-    Supplier must specify delivery time in the bid form.


C. REMARKS AND CONDITIONS

1. Providing, Supplying, and Transportation costs (loading and unloading) are included in the price.
2. Catalogues will be requested by GIZ during process for the needed items.
3. After awarding; a sample will be provided by supplier and GIZ will physically check and approve and the rest quantity will be provided after that.
4. In case any conflict between GIZ and supplier regarding the quality check of the product, Sulaymaniyah construction laboratory will be the reference to check the quality of the product.
[bookmark: _GoBack]
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