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Section II: Schedule of Requirements 
eSourcing reference: RFQ/2019/12557


Technical specifications for Goods and Comparative Data Table:

	Item No
	UNOPS minimum technical requirements
	Quantity
	Is quotation compliant? Bidder to complete
	Details of goods offered. Bidder to complete

	
	1) Manufacturer's Name 
2) Country of Origin
3) Brand /Model No
4) Year of Manufacture
	
	☐ Yes   ☐ No
	Please provide the details of offered product

	1
	25kva Generator (3 phase) set including the diesel engine, alternator, control panel, automatic starting equipment, fuel tank with a built-in canopy suitable for outdoor installation
	1
	☐ Yes   ☐ No
	Insert details (if required)

	1.1
	Engine
Fuel Type: Diesel 
Cooling: Water-cooled diesel Engine, 50˚C radiator cooled. 
Governor: Electric
Starting system: 24 Volt DC motor, lead acid battery with charging system. 
Speed: 1500 RPM, direct injection
No. of Strokes: 4

	
	☐ Yes   ☐ No
	Insert details (if required)

	1.2
	Output / Performance
Rating: 25KVA (Prime) 
Voltage: 220-415 Volts 
Frequency: 50 Hz 
( AVR ) : Automatic Voltage Regulator
	
	☐ Yes   ☐ No
	Insert details (if required)

	1.3
	Wiring & connectivity:
Connectivity of generator with main DB at the distance of 100 meter using suitable size of cable.
	
	☐ Yes   ☐ No
	Insert details (if required)

	1.4
	Warranty: One year from the date of start up
•Attend any minor service/repair/ breakdown within 6 hours upon request.
	
	☐ Yes   ☐ No
	Insert details (if required)

	1.5
	Canopy:
The generator set mounted in a sound attenuated and weather protective canopy,
	
	☐ Yes   ☐ No
	Insert details (if required)

	1.6
	Availability of spare parts and after sale service in Baghdad / Iraq 
	
	☐ Yes   ☐ No
	Insert details (if required)

	1.7
	Installation Fees 
	
	
	

	2
	ATS Panel:
Complete ATS (Automatic Transfer Switchboard (0-300 amps) 


	1
	☐ Yes   ☐ No
	Insert details (if required)




Delivery requirements and Comparative Data Table:

	UNOPS Requirements
	Is quotation compliant? Bidder to complete
	Details 
Bidder to complete

	Delivery time
	[bookmark: _GoBack]Bidder shall deliver the goods Two (2) weeks after Contract signature.
	☐ Yes   ☐ No
	Insert details 

	Delivery place and Incoterms rules
	                 DAP,
           Iraq, Baghdad 
UNMAS Office in Green Zone 
	☐ Yes   ☐ No
	Insert details 

	Consignee details
	Hanjuin Keka 
+964750 490 3415 
Hanjuink@unops.org 
	☐ Yes   ☐ No
	Insert details 

	UNOPS Right to vary requirements
	At the time the Contract is awarded, UNOPS reserves the right to vary the quantity of the goods and associated services specified above, provided this does not exceed +/- 20% , without any change in the unit prices or other terms and conditions of the RFQ.
	☐ Yes   ☐ No
	Insert details 
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