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Standard Specification to be met across all Lots for all vehicles


· New Unregistered vehicle
· Less than 6 months old from date of manufacture
· Less than 50 KM recorded in odometer
· Colour: White Solid Paint – No Stickers 
· Left Drive Vehicles
· Option a: Diesel Engine
· Option b: Petrol Engine
· Power to GVW ratio minimum 37 kW per tonne
· 4x4 All-wheel drive
· Option c: Manual 5-speed transmission minimum
· Option d: Automatic 5-speed transmission minimum
· High / Low range gearbox
· Seat Belts for all passengers and driver 
· Driver and Front passenger airbag
· Brakes (front/Rear) – Disc/Drum or disc
· Anti-Locking Brakes
· Suspension (front/rear) – Coil only/Leaf or coil
· Snorkel (optional)
· Tow Hook
· Fuel tank minimum 80 Litres minimum
· Air Conditioning 
· Radio 
· Emergency Kits (Fire extinguisher – First Aid Kit – Warning triangle)
· Basic Recovery Toolbox, including wheel brace 
· 12 Volt power  supply in front  (Remove Cigarette Lighter Socket)
· Front Electric Windows
· One Spare Tyre
· Warranty against manufacturing defects for a minimum of 20,000km or 1 year from date of acceptance, to include parts and labour

Additional mandatory specification for each Lot

Lot 1: 4x4 11 Seaters Hardtop Vehicle

· Minimum Payload of 1000 KG 
· 3 Doors 
· 11 Seats 3 (front) 2x4 Parallel Benches (rear), number of benches confirmed on order 
Toyota Landcruiser 70 series or any equivalent Models






Lot 2: 4x4 Double Cabin Pick-Up Vehicle

· 4 doors 
· 5 Seats minimum Configuration 
· Payload minimum 1,000 KG
Toyota Hilux or any equivalent model 

Lot 3: 4x4 7-Seater Vehicle

· 5 doors
· 7 Seats 
Toyota Prado or any equivalent model

Lot 4: People Carrier / Minibus

· 4 doors
· 9 places or above excluding driver



Optional Additional accessories to all lots

· Second Spare wheel and tyre
· Second Fuel Tank
· Heavy Duty Roof Rack 
· Hi Lift Jack with Platform/ Bottle Jack or equivalent 
· Heavy duty bull-bar with/without radio antenna predisposition
· HF/VHF radio
· Specific Sand Tyre upgrade
· 12v Portable Air Compressor (heavy duty) 
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