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Tdh is looking for the purchase vehicles with the following characteristics: 
	
	
	LOT 1 
	
	LOT 2

	
	TYPE OF VEHICLE
	SUV 
	
	PICK-UP DOUBLE CABIN 

	
	Conditions  
	New
	
	New

	
	Year
	Between of 2019 and 2021
	
	Between of 2019 and 2021

	
	Driver Wheel
	Left side
	
	Left side

	
	Wheeling drive
	4X4 & 4X2 
	
	4X4 & 4X2

	
	Numbers of seat
	7 seaters (02 in the front+ 05 in the back)
	
	5 seaters (2 in the front ,3 in the back)

	
	Max power HP/rpm
	150/3400
	
	150/3400

	
	Numbers of cylinders
	4 to 6
	
	4 to 6 

	
	Gear box
	Automatic or Manual
	
	Automatic or Manual

	
	Rear differential
	Standard
	
	Standard

	
	Brake
	ABS / SRS
	
	ABS / SRS

	
	Power steering
	YES
	
	YES

	
	Fuel type
	Benzene
	
	Benzene

	
	Fuel Tank Capacity
	Between 70 – 90L 
	
	Between 70 – 90L

	
	Payload 
	+/-1000 kg
	
	+/- 800 -1000  kg

	OPTIONS
	Air condition
	YES
	
	YES

	
	Airbags drivers and passengers
	YES
	
	YES

	
	Powered windows
	YES
	
	YES

	
	Stereo recorder and radio / USB Port
	YES
	
	YES

	
	 Model type or equivalent
	Model Type or equivalent: Chevrolet Trailblazer, GMC Acadia, Chevrolet Equinox, Kia Sorento
	
	Toyota Hilux, Mitsubishi L200, Nissan Navara, Ford ranger, GMC Canyon, Chevrolet Colorado…



The Model mentioned above are mainly given as information. 


All vehicle to be delivered with the equipment’s and tools mentioned in paragraph 2.2 in “instructions to tenderers”. The vehicles must be:

· Brand new, zero Km (mileage) 
· Registered in Iraq, before delivering to Tdh
· Custom cleared. Cost of the customs clearance (if imported) at the charge of the vendors
· Importation Tax cleared (if imported). Importation tax at the charge of the vendors
· Registered with ERBIL Plate Numbers
· Registration cost of  the car under Tdh name at the charge of the vendors. The registration must be issued by Iraq – Erbil traffic police directory) 
· Standard international vehicle warranty
· All vehicles shall be equipped with a fire extinguisher, first aid kit, spare wheel, basic tool kit, lift jack, triangle, seat belt in good condition.

Bidders and participants, who do not propose models that correspond exactly to the characteristics listed in the technical specifications, will have the opportunity to submit an offer for a model that comes as close as possible to the characteristics listed in the technical specifications
