[image: ]ANNEX 1 TECHNICAL SPECIFICATIONS
PN: 21.2116.8-001.00
Tender No: 91173714	
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A. TECHNICAL SPECIFICATIONS 

	Lot 1 

	No
	Item
	Description 
	Quantity 
	Reference Picture
	Comparative Specification
Comparative specification / remarks should indicate any deviation from technical parameter or functional description of tender specification or confirmation with "Yes" and if applicable further particularities.

	1. Electronic Supplies 

	1.1
	Supply and extend wires
	(2x2.5) mm² length (600 M.L). To connect electricity for interior switches with all requirements to cover all wires using PVC trunk wire size (25 mm). 2-4 wires in each PVC trunk
	600ml
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	1.2 
	Plug Socket Switches
	Supply and fix 13 Ampere , for one-stop-shop, type of switch contains Neon Light. Price includes all requirements for fitting all electricity works at One-stop-Shop counter.
	20pcs
	[image: ]

	[bookmark: Text2]     

	1. 3
	Supply and fix 10 Ampere Switch
	3 gangs two-way switch for fluorescent strip, work includes all requirements for fixing. 
Switches
	6pcs
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	2.
	Air Cooler 
	· Water tank capacity: 20 liters
· Blower function
· Rigid plastic body
· Cooling module 20000 m²/hr
· 1 channel
· 3-speed control
· Honeycomb cooling pad
· Air swingable for both sides, vertical and horizontal
· With an original remote control
· Movable and with 4 tires
· Proper pipe to be installed in order for the water reaches the cooling pads
	2pcs
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	3
	Wall mount fan
	· Motor: 14mm motor (motor size can be adjustable)
· Blade: 3 PP blade
· Voltage: 220V/50Hz
· Plug: Two round pin plug
· Color: Can be grey or black
· Body material type: PVC
	6pcs
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	4

	STORAGE WATER COOLERS
	· Capacity (40 LTR/HR)
· Storage capacity (80 LTR) 
· Of faucets 2 
· Dimensions (WXDXH) (665x 485 x 1210) mm (plus or minus 20 mm of the Dimensions are acceptable)
· Weight 45 Kg (plus or minus 2KG are acceptable)
· Refrigerant R22 /R 134A  
· Current amps are 2 
· Type of compressor ROTARY / RECIP
· Silver or White colour 
· Work includes all requirement to install water pipes, electricity sockets, draining
	1pcs
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	Lot 2

	No
	Item
	Description 
	Quantity 
	Reference Picture
	

	1
	Wooden desks
	· Classic type. Material made of lamination wood type HDF (High density fibres)
· Paper & veneer
· High gloss finish
· Colours brown or grey or red.
· Dimensions (LXWXH) mm (1400 X700 X740) mm 
· Three drawers’ size (5000 x4000 x5500) mm 
· Drawers with Key to be fixed to the desk 
· Hole/cord for computer cable and wires
	6pcs
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	2
	Office chair 

		· Moveable Leather office chair

	· Dimensions: 24.75"W x 27.25"
D x 38-40.5"H

	· Sit on smooth rolling multi- Surface dual 
wheel 
Casters 

	· Chrome base to provide easy
Access to your surrounding work 
         area 

	· Heavy-duty chair supports 
Up to 300 lbs 

	· Arm height adjustability allows
Precise arm Positioning and added
 hand (arms rest)

	· Wrist and forearm comfort 

	· Black color



	6pcs
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	3
	Fixed chair

		· Wood arm rest arm style

	· Seat &back Material leather

	· Seat Color black /brown

	· Weight Capacity approx. 225 Ib 

	· Chair frame steel

	· Seat Width 450 mm

	· Seat depth 480 mm

	· Height support 820 mm 

	· Cushion Thickness 3"



	30 pcs
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	4
	Fire extinguisher - Co2 fire extinguisher

		· Capacity 6 ± 0.15 

	· Fire rating 60 B 

	· Working temperature:
-20 C° ~ + 55 C° 

	· Rate pressure test 22.5 Mpa

	· Expiry date in best condition:
5 Years 


· 
	2 pcs
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B. WARRANTY & DOCUMENTS:  
· A minimum one-year warranty is required.





C. GENERAL REMARKS AND SPECIAL CONDITION

· Technical data sheets or catalogues are required for all items
· Pictures are only for understanding the product specifications, not indicative of a specific model or brand.
· All standard accessories for the offered items should be provided.
· The supplier must provide the items with all standard technical features and specifications, in full working condition.
· Packing, loading, transportation, and unloading are the responsibility of the supplier.
· The price should include transportation and installation costs.
· Suppliers can make an offer for one lot or both lots, provided that all items under the lot they offer for are provided.
· All dimensions are approximate, with a tolerance of plus or minus 20 mm.
· All items are subject to thorough checking and approval by the GIZ team and the recipients.

D. Delivery Location 
· The delivery location is Al-Rumaitha Municipality, allocated to the ONE STOP SHOP space.
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